TABLE 1Data available from sensors at Stations 1, 2 and 3

Parameter Units

Station 1 Station 2 and 3 0.1 s 1 s 60 s 300s 60 s 300s Sonic w m.s^{-1} - - - Sonic u m.s^{-1} - - - Sonic v m.s^{-1} - - - Sonic T_{c,} m.s^{-1} - - - Kr hygrometer q g.m^{-3} - - - Kr hygrometer relative humidity % - - - Kr hygrometer mixing ratio g Kg^{-1} - - - Kok ozone, mixing ratio ppbv - - - - SECL ozone, mixing ratio ppbv - - - - ThermoElectron ozone, mixing ratio ppbv - - - - Band pass hygrometer, temperature^o C

Band pass hygrometer, RH % Hygrothermometer, temperature^o C - - Hygrothermometer, relative humidity % - - Propvane, wind speed m.s^{-1} - - Propvane, wind direction^o Azimuth - - Barometric pressure mB - - Surface temperature^o C - - Net radiation W.m^{-2} - - Solar radiation W.m^{-2} - - Soil temperature^o C - - - - Soil heat flux W.m^{-2} - - - - Rain fall rate mm.s^{-1} - - - - Rainfall accumulation mm - - - - Momentum flux W.m^{-2} - - - - Sensible heat flux W.m^{-2} - - - - Latent heat flux W.m^{-2} - - - - Kok ozone flux g.m^{-2}.s^{-1} - - - - - SECL ozone flux g.m^{-2}.s^{-1} - - - - -